Just copy the SLIDE file inside the SERIAL folder to the main installation folder. No need to use a crack, however if the SLIDE file fails use the crack to make your own registering any serial. Again once a SLIDE file is made you don't need to use the crack at all.

Brains