
Lexmark Z51 Series ColorFine Printer Driver
for Microsoft Windows NT
----------------------------------------------------------

Tips:

 1) After you install the Lexmark Z51 Series software, the
    Lexmark Z51 Series ColorFine program group appears
    under Start/Programs.

 2) Many printing problems can be eliminated by setting
    Virtual Memory Initial Size to at least 128 MB. You
    should also set the Virtual Memory Maximum Size to
    at least 256 MB.

    Hint:  Click Start/Settings/Control Panel; double-click
    on System and go to the Performance tab; in the Virtual
    Memory section, select the Change button; change the
    Initial Size of the Paging File Size for Selected Drive;
    change the Maximum Size of the Paging File Size for
    Selected Drive; then press the Set button.

 3) This driver was designed to work best with the Default Datatype
    of LEMF. To select LEMF as the Print Processor Default Datatype:

    Click Start/Settings/Printers; right-click Lexmark Z51
    Series ColorFine printer icon, then click Properties.
    Click the Print Processor button.  Select the Lexmark
    Print Processor. Select LEMF as the Default Datatype.
    Click off "Always spool RAW datatype". Click OK.

 4) If DOS jobs fail to print:
    More than one printer driver may be installed on a PC.
    To correct the problem, attach all other printer drivers
    to FILE: as follows:
    1. Click Start/Settings/Printers.
    2. Right-click on the printer and select Properties.
    3. Go to the Ports tab and select FILE: from the list of ports.
    4. Click on OK.
    5. Repeat steps 2-4 for all printers except the Lexmark
       Z51 Series ColorFine.

 5) There are three different print quality modes in the driver
    ranging from a "draft" mode to a 1200 DPI mode. The
    differences between these modes are in the dots per inch
    addressed, and the number of passes of the print head used
    to apply ink to the print medium. The greater the number of
    passes, the higher the print quality.

    High Speed:      This is a 600x300 DPI high-speed "draft"
                     mode. All printing is done with one pass.
    Normal:          This is a 600x600 DPI mode. It is the
                     default for the driver. Printing is done
                     in either one or two passes, depending on
                     the print media used.
    High Quality:    This is the 1200x1200 DPI mode. All printing
                     is done in four passes.

 6) If you are unable to select 1200 Dots Per Inch (DPI) from
    within applications, you may select 1200 DPI mode
    from the driver.

    To get 1200 DPI mode from the driver for all documents:

      Click Start/Settings/Printers; right-click on the
      Lexmark Z51 printer icon; click Document Defaults;
      select High Quality; then click OK.

    To get 1200 DPI mode for a particular application:

      From the application's file menu, select Print, then Properties,
      Options, or Setup. Select High Quality; then click OK.

 7) If you select RAW as the Print Processor Default Datatype, then
    print jobs will not start printing until the last page is spooled.

 8) Peer-To-Peer printing works if the Peer's Print Processor
    Default Datatype is either RAW or LEMF.

 9) Full graphic Freehand files might print fastest with the Default
    Datatype of NT EMF. To select NT EMF as the Print Processor Default
    Datatype:

    Click Start/Settings/Printers; right-click Lexmark Z51
    Series ColorFine printer icon, then click Properties.
    Click the Print Processor button.  Select the Lexmark
    Print Processor. Select NT EMF as the Default Datatype.
    Click off "Always spool RAW datatype". Click OK.
