Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS) > How to Configure Your Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

### How to Configure Your Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)

1. Make sure that the power cord is plugged in and the top cover is closed.
2. Press to turn on the machine and make sure only the Ready LED ( ) lights up.
3. Press the Wi-Fi/WPS button three times.
4. The machine prints an eight-digit PIN and starts searching for a WLAN access point/router.
5. Using a computer that is on the network, type "http://access point's IP address" in your browser (where "access point's IP address" is the IP address of the device that is used as the Registrar).
6. Go to the WPS settings page and type the PIN, and then follow the on-screen instructions.
   - The Registrar is usually the wireless LAN access point/router.
   - The setting page will differ depending on the brand of wireless LAN access point/router. For more information, see the instructions supplied with your wireless LAN access point/router.

If you are using a Windows Vista®, Windows® 7, or Windows® 8 computer as a Registrar, complete the following steps:

7. Do one of the following:
   - (Windows Vista®)

     Click (Start)>Network>Add a wireless device.

   - (Windows® 7)

     Click (Start)>Devices and Printers>Add a device.

   - (Windows® 8)

     Move your mouse to the lower right corner of your desktop. When the menu bar appears, click Settings>Control Panel>Hardware and Sound>Devices and Printers>Add a device.

   - To use a Windows Vista®, Windows® 7, or Windows® 8 computer as a Registrar, you must register it to your network in advance. For more information, see the instructions supplied with your wireless LAN access point/router.
   - If you use Windows® 7 or Windows® 8 as a Registrar, you can install the printer driver after the wireless configuration by following the on-screen instructions. To install the full driver and software package, use the Fuji Xerox installer on the Installer CD-ROM.
8. Select your machine and click Next.
9. Type the PIN from the printed page, and then click Next.
10. Select your network, and then click Next.
11. Click Close.
12. If your wireless device is connected successfully, the Wi-Fi/WPS LED lights up and the machine prints your machine's wireless status report. If the connection fails, check the error code on the printed report.

    LED Indication | Setting WLAN *1 | Connected | Connection fail | No Access Point *2
    --- | --- | --- | --- | ---

    *1
    The LED will blink in a pattern of ON for 0.9 seconds and then OFF for 0.3 seconds.
    *2
    The LED will blink ON and OFF at 1.2 seconds intervals.

For Windows®:

You have completed the wireless network setup. To install drivers and software necessary for operating your device, click Install Printer Driver on the Installer CD-ROM's Top Menu page.

For Macintosh:

You have completed the wireless network setup. Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com/ to install drivers and software necessary for operating your device.

Related Information
  - Configure Your Machine for a Wireless Network Using the PIN Method of Wi-Fi Protected Setup™ (WPS)
  - Wireless LAN Report Error Codes

Go to top of page