Home > Network > Additional Methods of Configuring Your Fuji Xerox Machine for a Wireless Network > Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™ > How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

### How to Configure Your Wireless Network Using the One Push Method of WPS or AOSS™

1. Make sure that the power cord is plugged in and the top cover is closed.
2. Press to turn on the machine and make sure only the Ready LED ( ) lights up.
3. Press the WPS or AOSS™ button on your wireless access point/router.
4. Press and hold the Wi-Fi/WPS button on your machine for about two seconds.
5. The machine starts the one-push wireless setting mode.
   The machine will search for a WLAN access point/router that supports Wi-Fi Protected Setup or AOSS™ for two minutes.
6. If your wireless device is connected successfully, the Wi-Fi/WPS LED lights up and the machine prints your machine's wireless status report. If the connection fails, check the error code on the printed report.

   LED Indication | Setting WLAN *1 | Connected | Connection fail | No Access Point *2
   --- | --- | --- | --- | ---

   *1
   The LED will blink in a pattern of ON for 0.9 seconds and then OFF for 0.3 seconds.
   *2
   The LED will blink ON and OFF at 1.2 seconds intervals.

Related Information
  - Configure Your Machine for a Wireless Network Using the One Push Method of Wi-Fi Protected Setup™ (WPS) or AOSS™
  - Wireless LAN Report Error Codes

Go to top of page