TOSHIBA e-STUDIO Series

        Copyright(c) 2003-2012 TOSHIBA TEC CORPORATION All Rights Reserved.
                        Nov 08 2012

This product has the following restrictions and issues.  Please be sure to read this before using.

----------------------------------------------------------------------
<for Color Models>
        for Macintosh PPD(OS-X10.4.11 - 10.6.*)         Version 7.02
        for Macintosh PPD(OS-X10.7.* - 10.8.*)          Version 7.01
        for Macintosh PPD Plug-in(OS-X10.4.11 - 10.6.*) Version 7.01
        for Macintosh PPD Plug-in(OS-X10.7.* - 10.8.*)  Version 7.03

<for Black and White Models>
        for Macintosh PPD(OS-X10.4.11 - 10.6.*)         Version 7.01
        for Macintosh PPD(OS-X10.7.* - 10.8.*)          Version 7.01
        for Macintosh PPD Plug-in(OS-X10.4.11 - 10.6.*) Version 7.01
        for Macintosh PPD Plug-in(OS-X10.7.* - 10.8.*)  Version 7.03
----------------------------------------------------------------------

Issues
======

1. Macintosh Printing

- When printing is performed on Mac OS X 10.4.* to 10.8.*, AppleTalk cannot be used.

- When only Macintosh PPD file is installed without installing plug-in in Mac OS-X 10.7.* or later, a warning,"Some of the software for the printer is missing", appears at Add Printer.It is possible to print by pressing the "Continue" button on the warning display. 

- When a printer is added with IPP connection in Mac OS-X 10.8.* or later, a warning,"Unable to verify the printer on the Network" appears.It is possible to print by pressing the "Continue" button on the warning display. 

- Do not enter more than 10000 for size setting of the custom paper in Mac OS-X 10.8.* or later.
 
- All stapling options are displayed even though some are unavailable.  For example, you can select "Portrait A4 Left Hand Side" stapling even when you are using A3. As you cannot staple on the long edge of the A3, your job will not be stapled. However, the job will get printed.

- When using Macintosh and perform printing from an Adobe Acrobat PPD file on a paper of which size is other than Letter or A4 and the paper source to be used is specified, printing may be performed on Letter or A4 size paper fed from the Bypass Feeder.  When printing on a paper other than Letter or A4, set the paper source to Auto.

- Department Code "00000" is accepted on the Mac machine but not on the controller.

- When you designate the paper size in the page setting, the paper size such as A4 or Letter may not be displayed and "Others" may be displayed. In this case, the setting cannot be returned to "Others" if the size is changed to another one by clicking "OK". Or you can do this by designating another "Format for".

<e-STUDIO6550C Series>
- When you are using the MJ-1103 Finisher or MJ-1104 Saddle Stitch Finisher, copies cannot be stapled on Tray 1.

<e-STUDIO4540C Series / e-STUDIO456 Series>
- When you are using the MJ-1101 Finisher or MJ-1106 Saddle Stitch Finisher, copies cannot be stapled on Tray 1.

<e-STUDIO2550C Series / e-STUDIO5055C Series>
- When you are using the MJ-1107 Finisher or MJ-1108 Saddle Stitch Finisher, copies cannot be stapled on Tray 1.


--------------------------------------------------------------------------------
Trademarks
--------------------------------------------------------------------------------

- Apple, AppleTalk, Macintosh, Mac, TrueType, and LaserWriter are trademarks of Apple Inc. in the US and other countries.
- Postscript, and the brand names and product names of other Adobe Systems products are trademarks of Adobe Systems Incorporated in the US and other countries.
- TopAccess is a trademark of TOSHIBA TEC CORPORATION.
- Other company names and product names in this manual are the trademarks of their respective companies.
