Home > Network > Locate the Machine's Network Settings > Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

### Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

- Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com/ to download the latest version of BRAdmin Light.
- If you are using Windows® Firewall, or the firewall function of an anti-spyware or antivirus application, temporarily disable them. When you are sure you can print, configure the software settings following the instructions.
- Node name: The node name appears in the current BRAdmin Light window. The default node name is "BRWxxxxxxxxxxxx" (where "xxxxxxxxxxxx" is your machine's MAC Address / Ethernet address).
- No password is required by default. Type a password if you have set one.

1. Install BRAdmin Light.
2. Start BRAdmin Light.
   - (Windows® XP, Windows Vista®, Windows® 7, Windows Server® 2003 and Windows Server® 2008)

     Click (Start)>All Programs>Fuji Xerox>BRAdmin Light>BRAdmin Light.

   - (Windows® 8, Windows Server® 2012 and Windows Server® 2012 R2)

     Click (BRAdmin Light).

   - (Macintosh)

     Go to the download page for your model on the Fuji Xerox website at http://www.fujixeroxprinters.com/ to download the latest version of BRAdmin Light.

     Select the folder you have downloaded, and then double-click the BRAdmin Light.jar icon.

   BRAdmin Light will search for devices automatically.
3. Double-click on the print server whose settings you want to change.
   - If the print server is set to its factory default settings (if you do not use a DHCP/BOOTP/RARP server), the device will appear as Unconfigured in BRAdmin Light. Double-click the unconfigured device.
   - You can find the Node Name and MAC Address (Ethernet Address) by printing the Printer Settings Page.
4. Type a password if you have set one, and then click OK.

You can now change the network settings.

Related Information
  - Locate the Machine's Network Settings
  - Install BRAdmin Light from the Installer CD-ROM (Windows®)
  - Print the Printer Settings Page
  - Reset the Network Settings to the Factory Settings

Go to top of page