Home > Network > Troubleshooting > Identify and Solve the Problem > I Want to Check that My Network Devices are Working Correctly.

### I Want to Check that My Network Devices are Working Correctly.

Check | Action | Interface
--- | --- | ---
Check that your Fuji Xerox machine, access point/router, or network hub is turned on. | Check the following: The power cord is connected correctly and the Fuji Xerox machine is turned on. The access point/router or hub is turned on and its link button is blinking. All protective packaging has been removed from the machine. The toner cartridge and drum unit are installed correctly. The top cover is fully closed. Paper is inserted correctly in the paper tray. | Wireless
Check the Link Status in the Printer Settings Page. | Print the Printer Settings Page and check that Wireless Link Status is Link OK. | Wireless
Check that you can "ping" the Fuji Xerox machine from your computer. | Ping the Fuji Xerox machine from your computer using the IP address or the node name at the Windows® command prompt or Macintosh Terminal application: ping <ipaddress> or <nodename>. Successful: Your Fuji Xerox machine is working correctly and connected to the same network as your computer. Unsuccessful: Your Fuji Xerox machine is not connected to the same network as your computer. (Windows®) Ask the network administrator and fix the IP address and the subnet mask. (Macintosh) Confirm that the IP address and the Subnet Mask are set correctly. | Wireless
Check that your Fuji Xerox machine is connected to the wireless network. | Print the WLAN Report to check the error code on the printed report. | Wireless

If you have checked and tried all of the above but you are still having problems, see the instructions supplied with your wireless LAN access point/router to find the SSID and the Network Key information and set them correctly.

Related Information
  - Identify and Solve the Problem

Go to top of page