Home > Network > Advanced Network Features > Print the Printer Settings Page

### Print the Printer Settings Page

The Printer Settings Page lists the printer settings, including the network print server settings.

- Node Name: The Node Name appears on the Printer Settings Page. The default Node Name is "BRWxxxxxxxxxxxx" (where "xxxxxxxxxxxx" is your machine's MAC Address / Ethernet Address.)
- If the IP Address on the Printer Settings Page shows 0.0.0.0, wait for one minute and try printing it again.
- You can find your machine's settings, such as IP address, subnet mask, node name, and MAC Address on the settings page, for example:
  - IP address: 192.168.0.5
  - Subnet mask: 255.255.255.0
  - Node name: BRW000ca0000499
  - MAC Address: 00-0c-a0-00-04-99

1. Make sure that the power cord is plugged in and the top cover is closed.
2. Press to turn on the machine and make sure only the Ready LED ( ) lights up.
3. Press three times.
   The machine prints the Printer Settings Page.

Related Information
  - Advanced Network Features
  - Access Web Based Management
  - Locate Network Settings When Using Web Based Management
  - Locate Network Settings When Using BRAdmin Light (Windows® and Macintosh)

Go to top of page